The image oam_netinfo.png is a representation of the Oracle Appliance Manager Configurator Network Information screen. On the left side of the screen is a navigation field showing each installation screen name in sequence, with the Network Information screen field marked as the present screen. The preceding screens are shown with links. If you click the links, you can go directly back and forth to different pages. On the right side of the screen is a display of fields for network names and addresses for node1 and node2, with the following fields

Network Generic fields

- Domain name

- Name server IP

- NTP server IP

Network Specific Fields, showing IP address ranges where these addresses start

- ILOM interface IP address bond name, IP start range, and net mask

- Public, VIP and SCAN address bond name, IP start range, and net mask

- Net1 address bond name, IP start range, and net mask

- Net2 address bond name, IP start range, and net mask

- Net3 address bond name, IP start range, and net mask

Names and addresses generated for each node:

- Node1 and Node2 ILOM name and address

- Node1 and Node2 Public name and address

- Node1 and Node2 VIP name and address

- Node1 and Node2 Net1 name and address

- Node1 and Node2 Net2 name and address

- Node1 and Node2 Net3 name and address

In addition, for the cluster, there are fields for a SCAN name and two SCAN addresses. When you have completed entering the information for these screens, you click Next. There is additional description of this screen in the text following.