Screenshot arcight_config.gif shows the ArcSight SIEM page. From top to bottom, left to right, are the following components:

- Enable ArcSight event forwarding check box.

- Fields (top to bottom) for ArcSight destinations (UDP) and ArcSight destinations (TCP).

- Event categories: System, Alerts (selected by default), Info, Debug, and Heartbeat.

- Limit message length check box.

- Maximum message length (bytes).

- Apply and Cancel buttons.