This figure shows two VLAN blocks (1 and 2) of client systems. VLAN 1 contains two clients: A (IP address 10.161.48.628, MAC address 00-0C-H1-58-92-FG) and B (IP address 10.164.51.138, MAC address 00-0A-J4-23-65-CB). CLAN 2 contains one client: C (IP address 12.452.49.651, MAC address 00-0C-H1-56-92-FG). The connections (client and server ports) between them a two server VLAN blocks (1 and 2) are shown. Server VLAN 1 contains two servers: A (IP address 10.161.49.628, MAC address 00-0C-H1-58-92-FG), and B (IP address 10.164.51.138, MAC address 00-0A-J4-23-65-CB). Server VLAN block 2 contains one server: C (IP address 12.452.49.651, MAC address 00-0C-H1-58-92-FG).