Image okv_23a.png shows the High Availability Status page. From top to bottom, left to right, are the following components:

- The High Availability mode is enabled label

- From top to bottom, the Standby IP Address label and information (10.240.118.230), the High Availability Mode label and information (Primary), the Switchover Status label and information (TO STANDBY),, and the Standby system Certificate label and information (BEGIN_CERTIFICATE ...END CERTIFICATE)