## (area: "scef")

The _scef_ area includes all of the MMI APIs required for SCEF configuration which includes the following resources.

* NIDD Configuration Sets: A set of configurations that apply to NIDD call flows.
* APN Configuration Sets: A set of configurations that are associated to an APN, The APN is associated to a SCS/AS Profile.
* Monitoring Event Configuration Sets: A set of configurations for SCEF Monitoring Events.
* Device Triggering Configuration Sets: A set of configurations for Device Triggering to create a SCS/AS.
* SCS Application Servers: Service Capability Server (SCS) enables Applications to access and use functionality provided by Service Components over standardized interfaces (APIs).
* System Options: SCEF related user configurable Options.
* Access Control Lists: A set of configurations to support multi tenancy Access Control, DRMP and Flow/Overload Control during notification callback.
* Access Control Rules: A set of configurations to create an Access Control Rule.
* Access Control Associations: This is used to associate the Rules with an Access Control List.
