Syslog Setting indicates that you can enter IP addresses or hostnames as destinations, configure at least one DNS server before using hostnames. For TCP destinations the port number is also required and the UDP port defaults to 514.

There are the following fields with sample data:

Syslog Destinations (UDP): none

Syslog Destinations (TCP): 192.168.2.70:1522

192.168.2.58:1522

Select syslog categories to be selected. Check boxes are System, Alerts (checked), Info, Debug, and Heartbeat.

Lastly, there is an Apply button.