This image shows the layout of the servers and switches in the full rack. From the bottom to the top of the rack, the layout is as follows:

- Power Distribution Unit-B

- Power Distribution Unit-A

- Sun Datacenter QDR InfiniBand Switch (rear), 1U Vented Filler (front)

- U1 to U13: PDU A input 0, PDU B input 2

- U1 to U19: Big Data Appliance Servers, numbered from 1 through 9

- U14 to U28: PDU A input 1, PDU B input 1

- U20: Sun Network QDR InfiniBand Gateway (rear), 1U Vented Filler (front)

- U21: Cisco Ethernet Administration Switch (rear), 1U Vented Filler (front)

- U22: KVM Switch (rear), 1U Vented Filler (front)

- U23: KVM LCD

- U24: Sun Network QDR InfiniBand Gateway (rear), 1U Vented Filler (front)

- U25 to U42: Big Data Appliance Servers, numbered from 10 through 18

- U29 to U42: PDU A input 2, PDU B input 0